-Swap positive and negative terminals for XC60 connector - Fixed

-Resize footprint for ACS710\_R\_Sense - Fixed to be 1206 (3216)

-Resize relay footprint - Fixed

-Order stencil -

-Add QR Code, emails/contact info -

-Potentially change UART bridge -

-Potentially change Micro usb to B usb connector